|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Model** | | **AHA-373-DX** | **AHA-503-DX** | **AHA-603-DX** |
| **Capacity** | | **3.75KVA / 3KW** | **5KVA/4KW** | **6KVA/4.8KW** |
| Input | Voltage | single phase 220Vac -20% +35% | | |
| Frequency | 50Hz or 60Hz +/- 5% | | |
| Output | Voltage | single phase 220Vac +/- 5% (adjustable) | | |
| Frequency | 50Hz or 60Hz | | |
| Voltage Regulation | +/- 1% | | |
| Frequency Stability | +/- 0.5% (Free Running) | | |
| Transient Response | +/- 3% (100% load variation) | | |
| Waveform | Sinewave THD < 3% at 0-100% linear load | | |
| Overload Capacity | 120% load 30 seconds, >150% constant power. | | |
| Power factor | 0.7-1, lag | | |
| Crest ratio | 3 : 1 | | |
| Battery | Voltage | 192Vdc | | |
| Charger | 5A charger build in | | |
| Efficiency | AC to AC | >85% | | |
| Transfer Time | AC Fault | Zero | | |
| Protection | Battery | Battery low shutdown and breaker | | |
| Overload | 125% 30sec. switch to bypass line & automatic re-transfer | | |
| Short Circuit | Current Limited and cut-off and fuse and breaker | | |
| UPS Fault | Bypass, load supplied from mains less than 2ms. | | |
| EMI/EMC | EN50091-2, CE Approved | | |
| Audible Alarm | Mains Failure | Sounding every four seconds after mains fail, 90 seconds mute | | |
| Final Discharge | Sounding once every second as battery approaches | | |
| Overload | Continuously | | |
| UPS Fault | Continuously | | |
| Indicator | LCD | UPS state, I/P&O/P voltage, I/P&O/P frequency,  Battery voltage, Loading %,  History record | | |
|  | LED | Utility LED (green), Inverter LED (green), Battery Low (yellow)  Bypass voltage (yellow) Fault LED (red), Overload (yellow) | | |
| Interface | Contact Closure | Support MEGATEC RUPS UPS monitoring software | | |
| RS-232 | Support MEGATEC RUPSII / UPSilon 2000 monitoring software | | |
| Environment | Operation Temperature | 0-40 degree C; 32-104 degree F | | |
| Relative Humidity | 20-90% non-condensing | | |
| Audible Noise | Less than 45dB(at 1 meter) | | |
| Physical | Net Weight (KGS/LBs) | 69kgs without battery | | |
| Dimension (WxHxD)mm | 230 x 685 x 578 | | |

\* Specifications are subjected to change without prior notice.